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	Originating Party
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	ENVIRONMENTAL THRESHOLDS FOR LIQUID DISCHARGES AT SEA

	Author
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	Interface TQ - from
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	Type
	Query
	x
	Interface
	

	
	Deviation
	
	Derogation (SHALL[PS])
	

	
	Note: No deviations nor derogations which have an adverse effect on HSSE will be granted

	Workpackage
	SUMP CAISSON

	Area(s) of application
	Design & Eng.
	x
	Procurement
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	Operations
	
	Other
	

	Issue date
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	Urgent reply 5 days
	
	Routine reply 10 days
	x

	Close-out date
	17/09/23
	

	Closed-out by
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	Closed-out


	1. [bookmark: _Hlk14887621]Description 

	Reference documents / Aconex unique numbers:
“HSE Action Tracking Register and Close Out” Document No: K559-2254-SE-LST-001 

	Reference is made to FEED HAZID Action No. 7, which deals with the discharge of brine from process causing potential impact on marine life. In order to assess compliance with permitted liquid discharge limits at sea from the facility, COMPANY is requested to provide the applicable environmental limits as addressed in the Environmental Impact Assessment.



	2. Response

	Reference documents / Aconex unique numbers
Bijlage 3 Aanmeldnotitie m.e.r.-beoordeling BLPH.pdf

	With reference to Bijlage 3 Aanmeldnotitie m.e.r.-beoordeling BLPH.pdf, the applicable environmental limit is 2,500 kg/hour.

Translation, for information: For the production of hydrogen, per hour a maximum of 1,000 kg. fresh water is needed and for that about 3,000 kg/hour (circa 3.0 m3/hour) of sea water is pumped up. At the same time about 2,500 kg/hour (circa 2.5 m3/hour) of brine (sea water with a higher concentration of salts at around 28%) is discharched.

Original text, formal guidance: Voor de waterstofproductie is per uur maximaal 1000 kg zoet water nodig en daarvoor wordt ongeveer 3.000 kg/uur (ca. 3,0 m3/uur) zeewater opgepompt. Tegelijkertijd wordt er ongeveer 2.500 kg/uur (ca. 2,5m3/uur) pekelwater (zeewater met een hogere concentratie zouten van ca. 28%) geloosd.



This communication is issued for the recipient’s information and to facilitate the obligations
of the Parties under the Contract. This communication has no authority to amend                                                                      Page 2/2
or vary the Contract nor relieve either Party of any duties, obligations or responsibilities.								
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