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	Originating Party
	Rosetti Marino

	Subject
	Impressed Current Cathodic Protection Panel

	Author
	D. Lo Sterzo
	TQ Aconex unique number:  

	Interface TQ - from
	
	TQ interface source Aconex unique number:  



	Type
	Query
	x
	Interface
	

	
	Deviation
	
	Derogation (SHALL[PS])
	

	
	Note: No deviations nor derogations which have an adverse effect on HSSE will be granted

	Workpackage
	

	Area(s) of application
	Design & Eng.
	x
	Procurement
	
	Construction
	x

	
	Commissioning
	
	Operations
	
	Other
	

	Issue date
	10/10/2023
	Urgent reply 5 days
	x
	Routine reply 10 days
	

	Close-out date
	
	

	Closed-out by
	
	TQ status:
	Closed-out


	1. [bookmark: _Hlk14887621]Description 

	Reference documents / Aconex unique numbers:
Basic Design Engineering Package, doc. N. K559-2254-PM-PLN-003, sect. 9.7.7.4 ICCP

	Above referenced FEED requirement states that COMPANY will provide to Contractor an impressed current cathodic protection panel.
Company is kindly required to give all information needed for CONTRACTOR integration of this panel in plantform.
Minimum information to be received are:
· General arrangement drawings
· Single line diagram for Electrical connection
· Weight of the panel
· Transformer characteristics if any including Datasheet

	2. Response

	Reference documents / Aconex unique numbers
144671-CORR-TF-FAB-MRB-0001 ICCP System – Production - As Built

	· General arrangement drawings
· Power unit (144671-CORR-TF-FAB-DWG-0003, rev 5; pdf page 236/520)
· Step down Transformer Unit (see 144671-CORR-TF-FAB-DWG-0006, rev 5; pdf page 236/520)
· Junction box external system: (see 144671-CORR-TF-FAB-DWG-0011, Rev 2; pdf page 250/520)
· Junction box internal system: (see 144671-CORR-TF-FAB-DWG-0013, Rev 1; pdf page 254/520)

· Single line diagram for electrical connection
pdf page 216/520 to 223/520. Overview system diagram on pdf page 217/520
· Weight of the panel
· ICCP power unit 
· incl. frame: 165.86 kg (see 144671-CORR-TF-FAB-DWG-0006, rev 5; pdf page 236/520)
· excl. frame: 115.00 kg (see 144671-CORR-TF-FAB-DWG-0008, rev 0; pdf page 244/520)
· Step down transformer unit
· incl. frame: 154.71 kg: (see 144671-CORR-TF-FAB-DWG-0006, rev 5; pdf page 242/520)
· excl. frame: 118.12kg : (see 144671-CORR-TF-FAB-DWG-0015, rev 1; pdf page 258/520)
· Junction box external system:
· 10.62 kg: (see 144671-CORR-TF-FAB-DWG-0011, Rev 2; pdf page 250/520)
· Junction box internal system:
· 6.63 kg: (see 144671-CORR-TF-FAB-DWG-0013, Rev 1; pdf page 254/520)
· Transformer characteristics if any including datasheet
· Please refer to 144671-CORR-TF-FAB-MRB-0001 ICCP System – Production - As Built.
· 



This communication is issued for the recipient’s information and to facilitate the obligations
of the Parties under the Contract. This communication has no authority to amend                                                                      Page 2/2
or vary the Contract nor relieve either Party of any duties, obligations or responsibilities.								
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