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	Originating Party
	Rosetti Marino

	Subject
	BESS Process Information

	Author
	C. Impradice
	TQ Aconex unique number:  

	Interface TQ - from
	
	TQ interface source Aconex unique number:  



	Type
	Query x
	
	Interface x
	

	
	Deviation
	
	Derogation (SHALL[PS])
	

	
	Note: No deviations nor derogations which have an adverse effect on HSSE will be granted

	Workpackage
	

	Area(s) of application
	Design & Eng.
	x
	Procurement
	
	Construction
	

	
	Commissioning
	
	Operations
	
	Other
	

	Issue date
	21/09/2023
	Urgent reply 5 days
	x
	Routine reply 10 days
	

	Close-out date
	
	

	Closed-out by
	
	TQ status:
	Closed-out


	1. [bookmark: _Hlk14887621]Description 

	Reference documents / Aconex unique numbers:


	BESS Vendor is requested:

1)	to inform RM about process fluids type (H2, N2, Instrument Air and water or whatever), which are necessary for the proper working of the package (if any);
2)	to provide all process information (IN and OUT) of all fluids (operating and design conditions);
3)	to inform RM if a vent line outgoing from the package is present (if yes, then Vendor to inform RM about all process conditions on this stream).

	2. Response

	Reference documents / Aconex unique numbers


	The BESS package does not have any process interfaces.

There is one mechanical interface for the TR emergency exhaust vent. This will be detailed in the next revision of the general arrange drawing supplied by Statron





This communication is issued for the recipient’s information and to facilitate the obligations
of the Parties under the Contract. This communication has no authority to amend                                                                      Page 2/2
or vary the Contract nor relieve either Party of any duties, obligations or responsibilities.								
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