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	Originating Party
	Rosetti Marino

	Subject
	ICCP system

	Author
	Rosetti Marino – Electrical Department
	TQ Aconex unique number:  
ROSMA-INN-BPH-TQ-00079


	Interface TQ - from
	
	TQ interface source Aconex unique number:  

	Type
	Query
	X
	Interface
	

	
	Deviation
	
	Derogation (SHALL[PS])
	

	
	Note: No deviations nor derogations which have an adverse effect on HSSE will be granted

	Workpackage
	

	Area(s) of application
	Design & Eng.
	X
	Procurement
	
	Construction
	X

	
	Commissioning
	X
	Operations
	X
	Other
	

	Issue date
	14-mar-2024
	Urgent reply 5 days
	
	Routine reply 10 days
	X

	Close-out date
	
	

	Closed-out by
	
	TQ status:
	Closed-out


	1. [bookmark: _Hlk14887621]Description 

	Reference documents / Aconex unique numbers:
144671-CORR-TF-FAB-MRB-0001 ICCP System – Production - As Built

	As per reference document reported in this TQ and as discussed with CPY, contractor highlights that:
· Transformer 690/400V will not be installed.
· ICCP system control panel can be fed from 400V LV switchboard (SG-200)
· The ICCP control panel will be installed into a container.
· Anode’s JBs will be installed by CW on the transition piece, according to 144761-CORR-TF-FAB-DWG-0001 Rev.11 
(pdf page 217/520).
· Contractor will supply only the power cable to feed the ICCP control panel.
· Routing and connection of cabling between ICCP control panel and anode’s JBs to be done by Contractor.
[bookmark: _Hlk162433351]Contractor requests Company to acknowledge the above highlights related to interfaces between ICCP package and Contractor works.

	2. Response

	Reference documents / Aconex unique numbers


	Based on our recent discussions and meetings, the Company acknowledges the above dot points to be accurate and correct and Contractor’s updated technical details and scope of work represents what is required for the interface and installation of the ICCP package.




This communication is issued for the recipient’s information and to facilitate the obligations of the Parties under the Contract. This communication has no authority to amend or vary the Contract nor relieve either Party of any duties, obligations or responsibilities.						Page 1/1
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